# GTP Status Information for GGSN

The table displays the following information:

> GTP Version (cgprsGtpVersion)

> Last Non responding Peer GSN (cgprsGtpLastGSNidNoRespToEcho)

> Last Recovered Peer GSN (cgprsGtpLastGSNidRecovered)

> Unexpected PDP Context GSN (cgprsGtpGSNidOfLastUnexpPDPCxt)

> Unexpected PDP Context TID (cgprsGtpTIDOfLastUnexpPDPCxt)

> Last Rejection (cgprsGtpRejReasonOfLastUnexpPDPCxt)

### GTP Version (cgprsGtpVersion)

Indicates the GTP version supported by the device.

### Last Non responding Peer GSN (cgprsGtpLastGSNidNoRespToEcho)

Specifies the last peer GSN that did not reply to an echo message.

### Last Recovered Peer GSN (cgprsGtpLastGSNidRecovered)

Specifies the last peer GSN that did not reply to an echo message.

### Unexpected PDP Context GSN (cgprsGtpGSNidOfLastUnexpPDPCxt)

Specifies the peer GSN whose PDP context is unexpected.

### Unexpected PDP Context TID (cgprsGtpTIDOfLastUnexpPDPCxt)

The TID of the last unexpected PDP context activation.

### Last Rejection (cgprsGtpRejReasonOfLastUnexpPDPCxt)

Specifies the reason for rejecting the PDP context activation.