# Quota Managers

From this dialog box, you can view detail information (such as the IP address, port number, and current state) for the quota manager servers configured on the selected content services gateway (CSG) module.

## Navigation

1. Right-click the device, then select Configure > Content Services Gateway.

2. With a content services gateway (CSG) module selected, click Quota Managers.

The following information is displayed:

> IP Address (csgQuotaMgrIpAddr)

> Port Number (csgQuotaMgrPort)

> User-Group Name (csgQuotaMgrUserGroupName)

> Priority (csgQuotaMgrPriority)

> State (csgQuotaMgrState)

### IP Address (csgQuotaMgrIpAddr)

IP address of a quota manager.

### Port Number (csgQuotaMgrPort)

UDP port associated with a quota manager.

### User-Group Name (csgQuotaMgrUserGroupName)

Name of user group associated with a CSG module.

### Priority (csgQuotaMgrPriority)

Priority of a quota manager.

### State (csgQuotaMgrState)

States of a quota manager. There are six possible values:

> standby—The quota manager is ready to become active.

> failed—The quota manager has failed to respond to requests.

> active—The quota manager has been activated to receive requests.

> echowait—The CSG module has sent an echo request to this quota manager and is waiting for a response.

> nawait—The CSG module has sent a node-alive request to this quota manager and is waiting for a response.

> suspended—The quota manager has received a stop request from the operator.