# GGSN Access Point

The GGSN Access Point dialog box lists the IP addresses allocated to the MS.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Statistics.

4. Select GGSN Access Point Statistics from the Category drop-down box.

5. With an entry selected in the GGSN Access Point Statistics dialog box, click Monitor.

6. Select the category GGSN Access Point.

The following information is displayed:

> No. of IP Addresses Allocated (cgprsAccPtIpAddrAllocations)

> Total PDP Context (cgprsAccPtMsActivatedPdps)

> Successfully Completed PDP Context (cgprsAccPtSuccMsActivatedPdps)

> Dynamic PDP Context (cgprsAccPtMsActivatedDynPdps)

> Dynamic PDP Context Completed (cgprsAccPtSuccMsActivatedDynPdps)

> PDP Context Deactivation (cgprsAccPtMsDeactivatedPdps)

> PDP Context Deactivation Completed (cgprsAccPtSuccMsDeactivatedPdps)

### No. of IP Addresses Allocated (cgprsAccPtIpAddrAllocations)

Number of IP addresses allocated to the MS.

### Total PDP Context (cgprsAccPtMsActivatedPdps)

Total number of PDP context activation procedures initiated by any MS on this APN.

### Successfully Completed PDP Context (cgprsAccPtSuccMsActivatedPdps)

Total number of successfully completed PDP context activation procedures initiated by the MS on the APN.

### Dynamic PDP Context (cgprsAccPtMsActivatedDynPdps)

Total number of dynamic PDP context activation procedures initiated by the MS on the APN. When an MS requests dynamic PDP address from the PLMN, a dynamic PDP context activation procedure is initiated.

### Dynamic PDP Context Completed (cgprsAccPtSuccMsActivatedDynPdps)

Total number of successfully completed dynamic PDP context activation procedures initiated by the MS on the APN.

### PDP Context Deactivation (cgprsAccPtMsDeactivatedPdps)

Total number of PDP context deactivation procedures initiated by the MS on the APN.

### PDP Context Deactivation Completed (cgprsAccPtSuccMsDeactivatedPdps)

Total number of successfully completed PDP context deactivation procedures initiated by the MS.