# MIP(Mobile IP) System Group

The dialog box displays the following information:

MoIP Entities (mipEntities)

Enable MoIP (mipEnable)

Encapsulation Method (mipEncapsulationSupported)

### MoIP Entities (mipEntities)

Mobile entities supported by the managed entity.

Possible values are:

mobileNode (0)

foreignAgent (1)

homeAgent (2)

Note: The entity may support more than one Mobile IP entity. For example, the entity supports homeAgent (2) and foreignAgent (1) . Therefore, bit 1 and bit 2 are set to 1.

### Enable MoIP (mipEnable)

Indicates whether the Mobile IP protocol should be enabled for the managed entity.

Possible values are:

enabled (1) | MoIP is enabled for the managed entity.
disabled (2) | MoIP is disabled for the managed entity.

If MoIP is disabled, it should disable both agent discovery and registration functions.

### Encapsulation Method (mipEncapsulationSupported)

Encapsulation methods supported by the Mobile IP entity.

Possible values are:

ipInIp (0) | IP encapsulation within IP.
gre (1) | Generic routing encapsulation.
minEnc (2) | Minimal encapsulation within IP.
other (3) | Other.