# IGMP Snooping Capable Interfaces Rx Statistics

To access the IGMP Snooping Capable Interfaces Rx Statistics dialog box:

1. Select Device > Monitor > IGMP Snooping Statistics.

2. With an interface selected, click Monitor.

3. Select IGMP Snooping Capable Interfaces Rx Statistics.

This dialog box provides Rx statistics for IGMP Snooping capable interfaces.

The following data is displayed:

- General Queries Received (cisRxGeneralQueries)

- Group Specific Queries Received (cisRxGroupSpecificQueries)

- Total Membership Reports Received (cisRxReports)

- Total Membership Leaves Received (cisRxLeaves)

- Valid IGMP Packets Received (cisRxValidPackets)

- Invalid IGMP Packets Received (cisRxInvalidPackets)

- Valid Learning Queries and Messages Received (cisRxOtherPackets)

- Total MAC Based General Queries Received (cisRxMACGeneralQueries)

- Total Topology Notification Received (cisRxTopoNotifications)

The following list specifies buttons in this dialog box, as well as their function:

- To specify the refresh rate for this dialog box, select a value from the drop-down box.

- Click Start/Stop to begin/end device monitoring.

> Note: The Start/Stop toggle feature is supported only by CiscoView 5.x.

- Click Cancel to close the dialog box.

- Click Print to print the contents of the dialog box.

- Click Help to access online help.

General Queries Received (cisRxGeneralQueries)

Total number of general queries that have been received by an interface.

Group Specific Queries Received (cisRxGroupSpecificQueries)

Total number of group-specific queries that have been received by an interface.

Total Membership Reports Received (cisRxReports)

Total number of membership reports that have been received by an interface.

Total Membership Leaves Received (cisRxLeaves)

Total number of leave messages that have been received by an interface.

Valid IGMP Packets Received (cisRxValidPackets)

Total number of valid IGMP packets that have been received by an interface.

Invalid IGMP Packets Received (cisRxInvalidPackets)

Total number of packets which are not a valid IGMP messages received by an interface.

Valid Learning Queries and Messages Received (cisRxOtherPackets)

Total number of other valid IGMP message types (such as learning queries and messages) that have been received by an interface.

Total MAC Based General Queries Received (cisRxMACGeneralQueries)

Total number of MAC-based general queries that have been received by an interface.

Total Topology Notification Received (cisRxTopoNotifications)

Total number of topology notifications that have been received by an interface.