# CDMA PDSN Session Statistics

Use this option to view CDMA PDSN session details.

## Procedure

To access CDMA PDSN session information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN Session Table from the Category menu.

3. Select a row and click the Monitor button.

CDMA PDSN Session Table dialog box displays:

Data Octets Sent (cCdmaSessionSentOctets)

Data Octets Received (cCdmaSessionRcvdOctets)

Data Pkts Sent (cCdmaSessionSentPkts)

Data Pkts Received (cCdmaSessionRcvdPkts)

Outgoing Pkts Dropped (cCdmaSessionDiscardedOutPkts)

Incoming Pkts Dropped (cCdmaSessionDiscardedInPkts)

GRE Pkts Received (cCdmaSessionGREFromIPPkts)

GRE Pkts Sent (cCdmaSessionGREToIPPkts)

## Related Topics

CDMA PDSN Feature Overview

CDMA PDSN System Statistics

CDMA PDSN PCF Statistics

CDMA PDSN Session Statistics

Registration Statistics

RP Update Statistics Information

### Data Octets Sent (cCdmaSessionSentOctets)

The number of data octets sent to the mobile user since session established.

### Data Octets Received (cCdmaSessionRcvdOctets)

The number of data octets received from the mobile user since session established.

### Data Pkts Sent (cCdmaSessionSentPkts)

The number of data packets sent to the mobile user since session established.

### Data Pkts Received (cCdmaSessionRcvdPkts)

The number of data packets received from the mobile since session established.

### Outgoing Pkts Dropped (cCdmaSessionDiscardedOutPkts)

The number of outgoing data packets dropped by PDSN since system was last restarted.

### Incomming Pkts Dropped (cCdmaSessionDiscardedInPkts)

The number of incoming data packets dropped by PDSN since system was last restarted.

### GRE Pkts Received (cCdmaSessionGREFromIPPkts)

Number of GRE encapsulated packets received from IP since system was last restarted.

### GRE Pkts Sent (cCdmaSessionGREToIPPkts)

Number of GRE encapsulated packets delivered to IP for transmission since system was last restarted.