# PPP Setup Statistics

Use this option to view Packet Control Function (PCF) and Service Option (SO) based PPP Setup Statistics.

## Procedure

To access PPP Setup Statistics information:

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category menu.

3. Select any row and click PPP Setup Statistics.

The following information appears:

> Active Connections (cCdmaPcfSoPppCurrentConns)

> Connection Initiate Requests Sent (cCdmaPcfSoPppConnInitiateReqs)

> Successful Connections (cCdmaPcfSoPppConnSuccesses)

> Failed Connection Setup Requests (cCdmaPcfSoPppConnFails)

> Negotiations Aborted (cCdmaPcfSoPppConnAborts)

### Active Connections (cCdmaPcfSoPppCurrentConns)

Number of currently active PPP connections.

### Connection Initiate Requests Sent (cCdmaPcfSoPppConnInitiateReqs)

Number of PPP connection initiate Requests sent out since system startup.

### Successful Connections(cCdmaPcfSoPppConnSuccesses)

Number of PPP connections that were successfully brought to the active state since system startup.

### Failed Connection Setup Requests (cCdmaPcfSoPppConnFails)

Number of PPP connection setup Requests that have failed since system startup.

### Negotiations Aborted (cCdmaPcfSoPppConnAborts)

Since system startup,the number of PPP negotiations terminated prematurely due to an Mobile Node (MN) power-off .