# CDMA PDSN Traffic (Pkts) Statistics Contd

## Navigation

1. Right click the device, and select Monitor. The Monitor Device dialog box appears.

2. Select CDMA PDSN Traffic (Pkts) Statistics Contd from the Category list.

The following information appears:

> SDB Marked Data Packets (cCdmaTransmittedSDBPkts)

> GRE Key Missing Discarded Packets (cCdmaNoGREKeyPktDiscards)

> Session Not Found Discarded Packets (cCdmaNoSessionPktDiscards)

> GRE Protocol Discarded Packets (cCdmaInvGREProtoPktDiscards)

> Invalid Checksum Discarded Packets (cCdmaInvCheckSumPktDiscards)

### SDB Marked Data Packets (cCdmaTransmittedSDBPkts)

The total number of SDB marked data packets sent to PCF from PDSN since the system was last restarted.

### GRE Key Missing Discarded Packets (cCdmaNoGREKeyPktDiscards)

The total number of packets discarded from PCF because GRE Key is missing since the system was last restarted.

### Session Not Found Discarded Packets (cCdmaNoSessionPktDiscards)

The total number of packets discarded from PCF because the session is not found since the system was last restarted.

### GRE Protocol Discarded Packets (cCdmaInvGREProtoPktDiscards)

The total number of packets discarded from PCF because GRE protocol is invalid since the system was last restarted.

### Invalid Checksum Discarded Packets (cCdmaInvCheckSumPktDiscards)

The total number of packets discarded from PCF due to invalid checksum since the system was last restarted.