# Copy Software Image File

Device>Configure>File Copy>Copy Software Image File

Use the Copy Software Image File window to copy Software Image Files to and from a remote host to Flash memory. Use these settings:

Protocol (fileCopyProtocol)

TFTP or rcp for any remote copy.

From (fileCopyAction)

Use one of these options:

- Host to Flash Copy the image from host to the flash over the network through tftp/rcp.

- Flash to Host Copy the image from flash to host over the switch through tftp/rcp.

Remote Host IP Address (fileCopyRemoteServer)

IP address of tftp/rcp remote server from or to which to copy file.

Source File Name (fileCopySrcFileName)

Source filename (including the path, if applicable) of file.

Destination File Name (fileCopyDstFileName)

Destination filename (including path, if applicable) of file.

rcp User Name (fileCopyUserName)

Remote user name for copy via rcp.

Module Number (fileCopyModuleNumber)

The module number specified in the copy operation. This field is available only with intelligent modules (modules with their own images).