# SSG Excluded APN Table

The SSG Excluded APN Table category of the Configure dialog box displays details on the service selection gateway (SSG) excluded access point name (APN).

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG Excluded APN Table from the Category list.

The following information appears:

Excluded APN (cssgExcludedAPNName)

APN Row Status (cssgExcludedAPNRowStatus)

### Excluded APN (cssgExcludedAPNName)

Name of the excluded access point.

### APN Row Status (cssgExcludedAPNRowStatus)

Status of the table entry. You can use the status to add or delete a conceptual row in the table.

To create a row, set the object to createAndGo. There are no mandatory objects in a create request.

To delete a row, set the object to destroy.