-- This file was included in WWP MIB release 04-07-01-0008
-- file: RFC1215-TRAP.my
-- Changes:
--      Added MODULE definition.
--      Added IMPORTS.
-- dperkins@scruznet.com


RFC1215-TRAP DEFINITIONS ::= BEGIN


        IMPORTS
            snmp, ifIndex, egpNeighAddr
                    FROM RFC1213-MIB
            TRAP-TYPE
                    FROM RFC-1215;

        coldStart TRAP-TYPE
            ENTERPRISE  snmp
            DESCRIPTION
                "A coldStart trap signifies that the sending
                protocol entity is reinitializing itself such
                that the agent's configuration or the protocol
                entity implementation may be altered."
            ::= 0
  
        warmStart TRAP-TYPE
            ENTERPRISE  snmp
            DESCRIPTION
                "A warmStart trap signifies that the sending
                protocol entity is reinitializing itself such
                that neither the agent configuration nor the
                protocol entity implementation is altered."
            ::= 1

        linkDown TRAP-TYPE
            ENTERPRISE  snmp
            VARIABLES   { ifIndex }
            DESCRIPTION
                "A linkDown trap signifies that the sending
                protocol entity recognizes a failure in one of
                the communication links represented in the
                agent's configuration."
            ::= 2

        linkUp TRAP-TYPE
            ENTERPRISE  snmp
            VARIABLES   { ifIndex }
            DESCRIPTION
                "A linkUp trap signifies that the sending
                protocol entity recognizes that one of the
                communication links represented in the agent's
                configuration has come up."
        ::= 3

        authenticationFailure TRAP-TYPE
            ENTERPRISE  snmp
            DESCRIPTION
                "An authenticationFailure trap signifies that
                the sending protocol entity is the addressee
                of a protocol message that is not properly
                authenticated. While implementations of the
                SNMP must be capable of generating this trap,
                they must also be capable of suppressing the
                emission of such traps via an
                implementation-specific mechanism."
        ::= 4

        egpNeighborLoss TRAP-TYPE
            ENTERPRISE  snmp
            VARIABLES   { egpNeighAddr }
            DESCRIPTION
                "An egpNeighborLoss trap signifies that an EGP
                neighbor for whom the sending protocol entity
                was an EGP peer has been marked down and the
                peer relationship no longer obtains."
        ::= 5

END
