-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-VOIP-MIB.my
 --
 --

 WWP-VOIP-MIB DEFINITIONS ::= BEGIN

 IMPORTS 
   IpAddress, Integer32, OBJECT-TYPE, MODULE-IDENTITY, NOTIFICATION-TYPE
	FROM SNMPv2-SMI			
   DisplayString, MacAddress, TEXTUAL-CONVENTION			
	FROM SNMPv2-TC			
   wwpModules			
	FROM WWP-SMI;
	
	
 wwpVoipMIB MODULE-IDENTITY
       LAST-UPDATED "200104031700Z"
       ORGANIZATION "Ciena, Inc"
       CONTACT-INFO
	            "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com"
       DESCRIPTION
	       "This MIB module is for Voice Over IP feature 
               on WWP Products"
       REVISION     "200104031700Z"
       DESCRIPTION
               "Initial creation."
	 ::= { wwpModules 15 }
		
			
	
 --
 -- Node definitions
 --
	
 wwpVoipMIBObjects OBJECT IDENTIFIER ::= { wwpVoipMIB 1 }
	
 wwpVoip OBJECT IDENTIFIER ::= { wwpVoipMIBObjects 1 }

  -- Notifications 
  
 wwpVoipMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpVoipMIB 2 } 
 wwpVoipMIBNotifications       OBJECT IDENTIFIER ::=  
                       { wwpVoipMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpVoipMIBConformance OBJECT IDENTIFIER ::= { wwpVoipMIB 3 } 
 wwpVoipMIBCompliances OBJECT IDENTIFIER ::= { wwpVoipMIBConformance 1 } 		
 wwpVoipMIBGroups      OBJECT IDENTIFIER ::= { wwpVoipMIBConformance 2 }

		
 wwpVoipTable OBJECT-TYPE
     SYNTAX SEQUENCE OF WwpVoipEntry
     MAX-ACCESS     not-accessible
     STATUS         current
     DESCRIPTION
	     "The conceptual table listing all the Voice Over IP Entries."
     ::= { wwpVoip 1 }
		
 wwpVoipEntry OBJECT-TYPE
     SYNTAX WwpVoipEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
	"An entry in the wwpVoipTable."
     INDEX { wwpVoipIndex }
     ::= { wwpVoipTable 1 }
		
 WwpVoipEntry ::= SEQUENCE { 
     wwpVoipIndex               INTEGER,
     wwpVoipDownLoaderVersion   DisplayString,
     wwpVoipApplicationVersion  DisplayString,
     wwpVoipPortNum             INTEGER,
     wwpVoipIpAddr              IpAddress,
     wwpVoipNumResets           Integer32,
     wwpVoipCallAgentAddr       IpAddress,
     wwpVoipResetOp             INTEGER
 }

 wwpVoipIndex  OBJECT-TYPE
     SYNTAX       INTEGER(1..65535)
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "Index for the the Voip Entry."
     ::= { wwpVoipEntry 1 }
		
 wwpVoipDownLoaderVersion   OBJECT-TYPE
     SYNTAX       DisplayString
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "The Downloader version for this VOIP entry."
     ::= { wwpVoipEntry 2 }

 wwpVoipApplicationVersion   OBJECT-TYPE
     SYNTAX       DisplayString
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "The Aplication version for this VOIP entry."
     ::= { wwpVoipEntry 3 }

 wwpVoipPortNum   OBJECT-TYPE
     SYNTAX       INTEGER(1..65535)
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "The Port Number for the VOIP."
     ::= { wwpVoipEntry 4 }

 wwpVoipIpAddr    OBJECT-TYPE
     SYNTAX       IpAddress
     MAX-ACCESS   read-only
     STATUS       current
     DESCRIPTION
             "The IP Address for the VOIP Entry."
     ::= { wwpVoipEntry 5 }		
		
 wwpVoipNumResets OBJECT-TYPE
     SYNTAX          Integer32 (0..2147483647)
     MAX-ACCESS      read-only
     STATUS          current
     DESCRIPTION
	     "The number of times the VOIP processor has been reset."
     ::= { wwpVoipEntry 6 }
		
 wwpVoipCallAgentAddr OBJECT-TYPE
     SYNTAX          IpAddress
     MAX-ACCESS      read-only
     STATUS          current
     DESCRIPTION
	     "The IP address of the call agent to which this VOIP
             aplication is connected to."
     ::= { wwpVoipEntry 7 }

 wwpVoipResetOp     OBJECT-TYPE
     SYNTAX         INTEGER {
                         none(0),
                         reset(1)
                    }
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
	     "This object reset the VOIP Aplication. A read on this object
              always returns 'none'."
     ::= { wwpVoipEntry 8 }
		

 wwpVoipDiagFailNotification NOTIFICATION-TYPE
	STATUS	current
	DESCRIPTION
		"A wwpVoipDiagFailNotification is sent if T2 VOIP ASIC fails
                diagnostics."
	::= { wwpVoipMIBNotifications 1 }
 
	
 END

 --
 -- WWP-VOIP-MIB.my
 --
