-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-SYSTEM-CONFIG-MIB.my
 --

 WWP-LEOS-SYSTEM-CONFIG-MIB DEFINITIONS ::= BEGIN

 IMPORTS 		
   Unsigned32, OBJECT-TYPE, MODULE-IDENTITY			
	    FROM SNMPv2-SMI			
   DisplayString, TruthValue, DateAndTime, RowStatus, TEXTUAL-CONVENTION			
	    FROM SNMPv2-TC						
   wwpModules, 	wwpModulesLeos	
	    FROM WWP-SMI;
	
	
 wwpLeosSystemConfigMIB MODULE-IDENTITY
	    LAST-UPDATED "200203160000Z"
	    ORGANIZATION "Ciena, Inc"
	    CONTACT-INFO
		    "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com"
	    DESCRIPTION
		    "The MIB module for the WWP System Config information."
	    REVISION    "200203160000Z"
	    DESCRIPTION
		    "Initial creation."
	    ::= { wwpModulesLeos 12 }

 FileName ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "255a"
    STATUS       current
    DESCRIPTION
            "Represents the textual convention which defines the 
	     name string and display hint"
    SYNTAX       OCTET STRING (SIZE (1..64))

 --
 -- Node definitions
 --
	
 wwpLeosSystemConfigMIBObjects OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIB 1 }

 --
 -- SystemCfg Attributes
 --
 wwpLeosSystemConfigAttr OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBObjects 1 }

 --
 -- Cfg Group
 --
 wwpLeosSystemConfig OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBObjects 2 }
 
 --
 -- system telnet objects
 --
 wwpLeosSystemTelnet  OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBObjects 3 }
 
 -- Notifications 
  
 wwpLeosSystemConfigMIBNotificationPrefix  OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIB 2 } 
 wwpLeosSystemConfigMIBNotifications       OBJECT IDENTIFIER ::=  
                       { wwpLeosSystemConfigMIBNotificationPrefix 0 }

 -- Conformance information 
 
 wwpLeosSystemConfigMIBConformance OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIB 3 } 
 wwpLeosSystemConfigCompliances OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBConformance 1 } 		
 wwpLeosSystemConfigMIBGroups      OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBConformance 2 }
 				 		

 wwpLeosSystemConfigDefaultGateway OBJECT-TYPE
     SYNTAX      IpAddress
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
	     "Default gateway IP address."
     ::= { wwpLeosSystemConfigAttr 1 }

 wwpLeosSystemConfigBootCmdFile OBJECT-TYPE
      SYNTAX      FileName
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
	      "Name of the last successfully executed command file name 
	       executed by the device."
      ::= { wwpLeosSystemConfigAttr 2 }
      
 wwpLeosSystemConfigBootCfgFile OBJECT-TYPE
      SYNTAX      FileName
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
	      "This mib object specifies the bootup config file for the system.
	       Setting is object is similar to setting default load config file name.
	       When device will reboot it will attempt to load the file specified by 
	       wwpLeosSystemConfigBootCfgFile."
      ::= { wwpLeosSystemConfigAttr 3 }
 
 wwpLeosSystemClockDateTime    OBJECT-TYPE
     SYNTAX                DateAndTime
     MAX-ACCESS            read-write
     STATUS                current
     DESCRIPTION
	     "The current system date and time of box.  
				
	      There are no provisions for local time or
	      daylight savings. All times use the 24 hr clock
	      and are UTC.
				
	      Because device time is UTC, only first 7 bytes of
	      DateAndTime data are returned, as per RFC1903."
      ::= { wwpLeosSystemConfigAttr 4 }

 wwpLeosSystemConfigSavePermFile OBJECT-TYPE
      SYNTAX      FileName
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
	      "Setting this object will set the save file name 
	       to the value of wwpLeosSystemConfigSavePermFile.
	       What it means is that whenever wwpLeosSystemConfigControl
	       is set to value 'save' then if wwpLeosSystemConfigSaveFile is not set
	       then device will use wwpLeosSystemConfigSavePermFile as the file name
	       to store config."
      ::= { wwpLeosSystemConfigAttr 5 }

 wwpLeosSystemConfigLastFileNameReset OBJECT-TYPE
      SYNTAX      TruthValue
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
	      "Setting this object will reset the name of the last config
	       filename that was successfully executed by the device."
      ::= { wwpLeosSystemConfigAttr 6 }
 
 wwpLeosSystemServiceMode  OBJECT-TYPE
      SYNTAX      INTEGER {
      					none(0),
      					mpls(1),
      					pbt(2),
      					aoam(3)
      				}
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
	      "Setting this object will change the service mode of operation.
	       It will cause device to reboot. If this object is set to 'none' then 
	       device will reject the request and will return error."
      ::= { wwpLeosSystemConfigAttr 7 }    
      
 wwpLeosSystemConfigBackupGateway OBJECT-TYPE
     SYNTAX      IpAddress
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
	     "Backup gateway IP address."
     ::= { wwpLeosSystemConfigAttr 8 }
     
 wwpLeosSystemConfigCustomerCfgFile OBJECT-TYPE
      SYNTAX      FileName
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
	      "Setting this object will set the name of the default customer configuration
	       file name, which is the file that will copied to the default configuration
	       file during a reset-to-customer-default operation.  Setting this object to
	       an empty string will remove the file name from the system configuration."
      ::= { wwpLeosSystemConfigAttr 9 }

      
 wwpLeosSystemConfigSaveFileName OBJECT-TYPE
      SYNTAX		FileName
      MAX-ACCESS	read-write
      STATUS		current   
      DESCRIPTION
	      "wwpLeosSystemConfigSaveFileName specifies the name of the config
	       file to be used when wwpLeosSystemConfigControl has been set 
	       to 'save'. If this object is not set then device will use 
	       the file name specified by wwpLeosSystemConfigSavePermFile.
	       If wwpLeosSystemConfigSavePermFile is also not set then default config 
	       file name i.e startup-config will be used to save config.
	       Once 'wwpLeosSystemConfigControl' has been successfully applied,
	       read on wwpLeosSystemConfigSaveFileName will always return empty
	       string else it will show what user has configured."
       ::= { wwpLeosSystemConfig 1 }
       
 wwpLeosSystemConfigControl OBJECT-TYPE
      SYNTAX          INTEGER {
                           none(0),
			   save(1),   
			   mfgDefaultCfg(2)
		       }
      MAX-ACCESS       read-write
      STATUS           current   
      DESCRIPTION
	      "Controls configuration options on the device.
              The current options are:
	      save:   
		  to make the configuration changes made
		  using SNMP persistent across a reboot.
				 
	      mfgDefaultCfg:
		   Set system configuration to factory defaults.
		   Note: this will wipe out all of the current 
		   configuration including Password and VLAN 
		   information.
              
             If the system doesn't support any of these control 
             configuration option, it should return error while 
             trying to set this object to the specific option.
              
             A read on this object should return none(0)."
       ::= { wwpLeosSystemConfig 2 }
 
 wwpLeosSystemConfigFilepath OBJECT-TYPE
      SYNTAX        FileName
      MAX-ACCESS    read-only
      STATUS        current
      DESCRIPTION
	      "Returns the path for configuration related files."
      ::= { wwpLeosSystemConfig 3 }
 				
 --
 --  The System Config File Table
 --

 wwpLeosSystemConfigFileTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosSystemConfigFileEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "The (conceptual) table listing the configs"
     ::= { wwpLeosSystemConfig 4 }

 wwpLeosSystemConfigFileEntry OBJECT-TYPE
    SYNTAX     WwpLeosSystemConfigFileEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "An entry (conceptual row) in the wwpLeosSystemConfigFileTable."
    INDEX      { wwpLeosSystemConfigFileIndex }
    ::= { wwpLeosSystemConfigFileTable 1 }


 WwpLeosSystemConfigFileEntry ::= SEQUENCE {
    wwpLeosSystemConfigFileIndex      INTEGER,   
    wwpLeosSystemConfigFileName       FileName,
    wwpLeosSystemConfigActivateFile   INTEGER
 }
 
 wwpLeosSystemConfigFileIndex     OBJECT-TYPE
     SYNTAX             INTEGER(1..65535)
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
    	     "Unique identifier to the table."               
     ::= { wwpLeosSystemConfigFileEntry 1 }
 
 wwpLeosSystemConfigFileName     OBJECT-TYPE
     SYNTAX          FileName
     MAX-ACCESS      read-only
     STATUS          current
     DESCRIPTION
    	     "The name of the Config file."               
     ::= { wwpLeosSystemConfigFileEntry 2 }
 
 wwpLeosSystemConfigActivateFile  OBJECT-TYPE
     SYNTAX      INTEGER {
		     loadCfg(1),
		     resetToCfg(2),
		     none(3)
		 }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
	     "Set this object to 'loadCfg to load the 'wwpLeosSystemConfigFileName' config. 
	      If the operation was successful, this object performs 
              the CLI equivalent to these commands and will return the status
	      
	      Setting this object to 'resetToCfg' will kills the load module and reloads a new load module and 
	      applies the config file specified by wwpLeosSystemConfigFileName.
	      
	      Setting this object to none will do nothing."  
	  DEFVAL {none}
     ::= { wwpLeosSystemConfigFileEntry 3 }
     
 wwpLeosTelnetMaxBaseUserSessions OBJECT-TYPE
     SYNTAX           INTEGER (0..10)      
     MAX-ACCESS       read-write
     STATUS           current   
     DESCRIPTION
             "The max number of base user telnet sessions
             for the device."
     ::= { wwpLeosSystemTelnet 1 }
     
 wwpLeosTelnetMaxSuperUserSessions OBJECT-TYPE
     SYNTAX           INTEGER (0..10)
     MAX-ACCESS       read-write
     STATUS           current   
     DESCRIPTION
             "The max number of super user telnet sessions
             for the device."
     ::= { wwpLeosSystemTelnet 2 }    

 --
 -- System Cpu Load Query
 --
 wwpLeosSystemCpuLoadQuery OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBObjects 7 }

 wwpLeosSystemCpuLoad1Min OBJECT-TYPE
     SYNTAX     INTEGER(1..65535)
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
            "The OID to display CPU load in last 1 min."
     ::= { wwpLeosSystemCpuLoadQuery 1 }

 wwpLeosSystemCpuLoad10Min OBJECT-TYPE
     SYNTAX     INTEGER(1..65535)
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
            "The OID to display CPU load in last 10 min."
     ::= { wwpLeosSystemCpuLoadQuery 2 }
 
 wwpLeosSystemCpuLoad15Min OBJECT-TYPE
     SYNTAX     INTEGER(1..65535)
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
            "The OID to display CPU load in last 15 min."
     ::= { wwpLeosSystemCpuLoadQuery 3 }

 wwpLeosSystemCpuLoad5Min OBJECT-TYPE
     SYNTAX     INTEGER(1..65535)
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
            "The OID to display CPU load in last 5 min."
     ::= { wwpLeosSystemCpuLoadQuery 4 }
 
 --
 -- String used for notification
 --
 wwpLeosSystemConfigNotif OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBObjects 8 }

 wwpLeosSystemConfigNotifTable OBJECT-TYPE
     SYNTAX     SEQUENCE OF WwpLeosSystemConfigNotifEntry
     MAX-ACCESS not-accessible
     STATUS     current
     DESCRIPTION
            "The (conceptual) table listing the configuration file line numbers.
	     This table is only used when sending wwpLeosImproperCmdInConfigFile
	     notification. No Get, GetNext or Set is allowed on this table."
     ::= { wwpLeosSystemConfigNotif 1 }

 wwpLeosSystemConfigNotifEntry OBJECT-TYPE
    SYNTAX     WwpLeosSystemConfigNotifEntry
    MAX-ACCESS not-accessible
    STATUS     current
    DESCRIPTION
            "An entry (conceptual row) in the wwpLeosSystemConfigNotifTable.
	     No Get, GetNext or Set is allowed on this table."
    INDEX      { wwpLeosSystemConfigFileIndex }
    ::= { wwpLeosSystemConfigNotifTable 1 }

 WwpLeosSystemConfigNotifEntry ::= SEQUENCE {
    wwpLeosSystemConfigErrLineNum	INTEGER,
    wwpLeosSystemConfigErrStr		DisplayString,
    wwpLeosSystemConfigErrLinesTotal	INTEGER
 }

 wwpLeosSystemConfigErrLineNum OBJECT-TYPE
     SYNTAX     INTEGER (0..64)
     MAX-ACCESS read-only
     STATUS     current
     DESCRIPTION
            "The OID is sent in the wwpLeosImproperCmdInConfigFile 
	     trap to identify the line number which was failed 
	     when configuration is applied. No Get, GetNext or Set is 
	     allowed on this table."
     ::= { wwpLeosSystemConfigNotifEntry 1 }
     
     
 wwpLeosSystemConfigErrStr OBJECT-TYPE
          SYNTAX      DisplayString
          MAX-ACCESS  read-only
          STATUS      current
          DESCRIPTION
                 "The OID is  wwpLeosSystemConfigErrStr
     	     trap to identify the line  which was failed 
     	     when configuration is applied. No Get, GetNext or Set is 
     	     allowed on this table."
    ::= { wwpLeosSystemConfigNotifEntry 2 }
    
    
 wwpLeosSystemConfigErrLinesTotal OBJECT-TYPE
         SYNTAX     INTEGER (0..64)
         MAX-ACCESS read-only
         STATUS     current
         DESCRIPTION
                "The OID is sent in the wwpLeosImproperCmdInConfigFile 
    	     trap to identify the total line numbers which was failed 
    	     when configuration is applied. No Get, GetNext or Set is 
    	     allowed on this table."
     ::= { wwpLeosSystemConfigNotifEntry 3 }
     
 --
 -- System Memory Usage
 --
 wwpLeosSystemMemoryUsageQuery OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBObjects 9 }

 wwpLeosSystemMemoryUsageTable OBJECT-TYPE
        SYNTAX          SEQUENCE OF WwpLeosSystemMemoryUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "Table of Memory Usage for various Memory Pools."
        ::= { wwpLeosSystemMemoryUsageQuery 1 }
        
 wwpLeosSystemMemoryUsageEntry OBJECT-TYPE
        SYNTAX          WwpLeosSystemMemoryUsageEntry
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "An entry for each Memory Pool."
        INDEX { wwpLeosSystemMemoryUsagePoolIndex }
        ::= { wwpLeosSystemMemoryUsageTable 1 }
        
 WwpLeosSystemMemoryUsageEntry ::= SEQUENCE {
        wwpLeosSystemMemoryUsagePoolIndex       INTEGER,
        wwpLeosSystemMemoryUsageMemoryTotal     Unsigned32,
        wwpLeosSystemMemoryUsageMemoryLWM       Unsigned32,
        wwpLeosSystemMemoryUsageMemoryFree      Unsigned32,
        wwpLeosSystemMemoryUsageStatus          INTEGER,
	wwpLeosSystemMemoryUsageMemoryUsed      Unsigned32,
	wwpLeosSystemMemoryUsageMemoryAvailable Unsigned32
 }
 
 wwpLeosSystemMemoryUsagePoolIndex OBJECT-TYPE
        SYNTAX          INTEGER {
                                ose-pool-1      (1),    -- OSE Pool 1
                                global-heap     (2),    -- Global Heap
                                malloc-heap		(3) 	-- Malloc Heap
                        }
        MAX-ACCESS      not-accessible
        STATUS          current
        DESCRIPTION     "The Memory Pool type."
        ::= { wwpLeosSystemMemoryUsageEntry 1 }
        
 wwpLeosSystemMemoryUsageMemoryTotal OBJECT-TYPE
        SYNTAX          Unsigned32
        UNITS           "bytes"
        MAX-ACCESS      read-only 
        STATUS          current
        DESCRIPTION     "Total size of the Memory Pool in bytes."
        ::= { wwpLeosSystemMemoryUsageEntry 2 }
        
 wwpLeosSystemMemoryUsageMemoryLWM OBJECT-TYPE
        SYNTAX          Unsigned32
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "Lowest free memory in the Memory Pool in bytes.
			Not supported in SAOS 6.x"
        ::= { wwpLeosSystemMemoryUsageEntry 3 }

 wwpLeosSystemMemoryUsageMemoryFree OBJECT-TYPE
        SYNTAX          Unsigned32
        UNITS           "bytes"
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "Amount of free memory in the Memory Pool in bytes.
			This correspondes the CLI's memory never used"
        ::= { wwpLeosSystemMemoryUsageEntry 4 }

 wwpLeosSystemMemoryUsageStatus OBJECT-TYPE
        SYNTAX          INTEGER  {
                                 normal(1),
                                 lowMemory(2),
                                 notSupported(3)
                        }
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "Denotes if the free memory amount is normal or below limit."
        ::= { wwpLeosSystemMemoryUsageEntry 5 }

wwpLeosSystemMemoryUsageMemoryUsed OBJECT-TYPE
        SYNTAX          Unsigned32
        UNITS           "bytes"
        MAX-ACCESS      read-only  
        STATUS          current
        DESCRIPTION     "Amount of used memory in the Memory Pool in bytes.."
        ::= { wwpLeosSystemMemoryUsageEntry 6 }

wwpLeosSystemMemoryUsageMemoryAvailable OBJECT-TYPE
        SYNTAX          Unsigned32
        UNITS           "bytes"
        MAX-ACCESS      read-only
        STATUS          current
        DESCRIPTION     "Amount of avaliable memory in the Memory Pool in bytes."
        ::= { wwpLeosSystemMemoryUsageEntry 7 }
 --
 -- xFTP 
 --
wwpLeosSystemXFtp OBJECT IDENTIFIER ::= { wwpLeosSystemConfigMIBObjects 10 }

 wwpLeosSystemXFtpMode  OBJECT-TYPE
      SYNTAX      INTEGER {
      				tftp(1),
      				ftp(2),
      				sftp(3)
      		          }
      MAX-ACCESS  read-write
      STATUS      current
      DESCRIPTION
	      "Select between modes of file transfer.
               The default mode is tftp."
      ::= { wwpLeosSystemXFtp 1 }    

 wwpLeosSystemXFtpServer OBJECT-TYPE
     SYNTAX      DisplayString 
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
	     "IP address or the host name of default server."
     ::= { wwpLeosSystemXFtp 2 }


 wwpLeosSystemXFtpUserName OBJECT-TYPE
     SYNTAX       DisplayString(SIZE(0..254)) 
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
	     "Name used to login with."
     ::= { wwpLeosSystemXFtp 3 }

 wwpLeosSystemXFtpPasswd OBJECT-TYPE
     SYNTAX       DisplayString(SIZE(0..128)) 
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
	     "Password used to login with."
     ::= { wwpLeosSystemXFtp 4 }


 wwpLeosSystemXFtpNumOfRetries OBJECT-TYPE
     SYNTAX      INTEGER(1..10) 
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
	     "Number of times to retry a file transfer request if it fails."
     ::= { wwpLeosSystemXFtp 5 }

 wwpLeosSystemXFtpRetryInterval OBJECT-TYPE
     SYNTAX      INTEGER(1..300) 
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
	     "Length of time in seconds to wait before retrying a file transfer if it fails."
     ::= { wwpLeosSystemXFtp 6 }

 wwpLeosSystemXFtpConnectionTimeout OBJECT-TYPE
     SYNTAX      INTEGER(1..100) 
     MAX-ACCESS   read-write
     STATUS       current
     DESCRIPTION
	     "Length of time in seconds to wait before connection times out."
     ::= { wwpLeosSystemXFtp 7 }

 --
 -- Traps
 --

 wwpLeosImproperCmdInConfigFile  NOTIFICATION-TYPE
	OBJECTS	   {  
	              wwpLeosSystemConfigFileName, 
		      wwpLeosSystemConfigErrLineNum,
		      wwpLeosSystemConfigErrLinesTotal
		      
		   }
	STATUS	   current
	DESCRIPTION  
		"A wwpLeosImproperCmdInConfigFile notif signifies that the SNMP entity, acting in
                an agent role, has counted the number of improper commands that  were found in the
		configuration file while processing the wwpLeosSystemConfigFileName"  
	::= { wwpLeosSystemConfigMIBNotifications 1 } 
	
 wwpLeosSystemServiceModeChange  NOTIFICATION-TYPE
	OBJECTS	   {  
	              wwpLeosSystemServiceMode		      
		   	   }
	STATUS	   current
	DESCRIPTION  
		"A wwpLeosSystemServiceModeChange notification will be sent out whenever someone changes the system service mode 
		 between mpls and pbt."  
	::= { wwpLeosSystemConfigMIBNotifications 2 }

 wwpLeosSystemMemoryStatusNotification  NOTIFICATION-TYPE
	OBJECTS	   {  
	              wwpLeosSystemMemoryUsageMemoryTotal,
	              wwpLeosSystemMemoryUsageMemoryFree,
	              wwpLeosSystemMemoryUsageStatus,
                      wwpLeosSystemMemoryUsageMemoryAvailable
		   	   }
	STATUS	   current
	DESCRIPTION  
		"A wwpLeosSystemMemoryStatusNotification notification will be sent out whenever the system memory is
		 below threshold limit."  
	::= { wwpLeosSystemConfigMIBNotifications 3 }   
	
 wwpLeosImproperCmdInConfigLineString  NOTIFICATION-TYPE
	OBJECTS	   {  
	                  wwpLeosSystemConfigErrStr,
	                  wwpLeosSystemConfigErrLineNum,
	                  wwpLeosSystemConfigFileName
		   }
		   
	STATUS	   current
	DESCRIPTION  
		"A wwpLeosImproperCmdInConfigLineString notif signifies that the SNMP entity, acting in
                an agent role, has detected that improper commands were found in the
		configuration file while processing the wwpLeosSystemConfigFileName. 
		wwpLeosSystemConfigErrStr will specify the commands which failed with the line number."  
	::= { wwpLeosSystemConfigMIBNotifications 4 } 
        
 END
     
 --
 -- WWP-SYSTEM-CONFIG-MIB.my
 --
