-- This file was included in WWP MIB release 04-07-01-0008
 --
 -- WWP-LEOS-TWAMP-MIB.my
 --
 --

 WWP-LEOS-TWAMP-MIB DEFINITIONS ::= BEGIN

 IMPORTS 		
     Integer32, Unsigned32, OBJECT-TYPE, MODULE-IDENTITY			
	    FROM SNMPv2-SMI
     TruthValue, DateAndTime, DisplayString
            FROM SNMPv2-TC
     wwpModules, wwpModulesLeos		
	    FROM WWP-SMI;	

 wwpLeosTwampMIB MODULE-IDENTITY
	    LAST-UPDATED "200802150800Z"
	    ORGANIZATION "Ciena, Inc"
	    CONTACT-INFO
		    "   Mib Meister
		  			115 North Sullivan Road
					Spokane Valley, WA 99037
		        	USA		 		
		        	Phone:  +1 509 242 9000
					Email:  support@ciena.com"    
		DESCRIPTION
			"Added wwpLeosTwampClientSessionsTable under wwpLeosTwampModule
			 Added wwpLeosTwampClientSessionsStatisticsTable under wwpLeosTwampModule."
		REVISION  "200808080800Z"
	    DESCRIPTION
		    "The MIB module for the WWP Specifc twamp mib. It contains the 
                     variables which applies to TWAMP functionality on the chassis for the WWP System."
	    REVISION    "200802150800Z"
	    DESCRIPTION
		    "Initial creation."
	    ::= { wwpModulesLeos 40 }

 
 --
 -- Node definitions
 --
	
 wwpLeosTwampMIBObjects OBJECT IDENTIFIER ::= { wwpLeosTwampMIB 1 }
 
 wwpLeosTwamp OBJECT IDENTIFIER ::= { wwpLeosTwampMIBObjects 1 }
 
  -- the Twamp Module 

 wwpLeosTwampModule OBJECT IDENTIFIER ::= { wwpLeosTwamp 1 } 

  wwpLeosTwampPort OBJECT-TYPE
     SYNTAX             INTEGER (256..65535)
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TCP/UDP port for TWAMP messaging."
     ::= { wwpLeosTwampModule 1 }   
     
  wwpLeosTwampEnable OBJECT-TYPE
     SYNTAX             INTEGER {
                            disable(0),
                            enable(1)
                        }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "System level TWAMP enable/disable."
     ::= { wwpLeosTwampModule 2 }   

 --
 -- TWAMP Port enable/disable
 --
 wwpLeosTwampPortEnableTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTwampPortEnableEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of Ethernet Ports Traps."
     ::= { wwpLeosTwampModule 3 }
                
 wwpLeosTwampPortEnableEntry OBJECT-TYPE
     SYNTAX       WwpLeosTwampPortEnableEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "TWAMP enable state of the port."
     INDEX { wwpLeosTwampPortId }
     ::= { wwpLeosTwampPortEnableTable 1 } 

 WwpLeosTwampPortEnableEntry ::= SEQUENCE { 
     wwpLeosTwampPortId              INTEGER,
     wwpLeosTwampPortEnableState     INTEGER     
  } 

 wwpLeosTwampPortId     OBJECT-TYPE
     SYNTAX             INTEGER (1..28)
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Port index for TWAMP messaging."
     ::= { wwpLeosTwampPortEnableEntry 1 }   
     
 wwpLeosTwampPortEnableState   OBJECT-TYPE
     SYNTAX         INTEGER {
                        disable(0),
                        enable(1)
                    }
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
             "Setting this object will enable or disable TWAMP messaging on given port."
     ::= { wwpLeosTwampPortEnableEntry 2 }
     
  wwpLeosTwampClientEnable OBJECT-TYPE
     SYNTAX             INTEGER {
                            disable(0),
                            enable(1)
                        }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TWAMP Client enable/disable."
     ::= { wwpLeosTwampModule 4 }   

  wwpLeosTwampServerEnable OBJECT-TYPE
     SYNTAX             INTEGER {
                            disable(0),
                            enable(1)
                        }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TWAMP Server enable/disable."
     ::= { wwpLeosTwampModule 5 }   

  wwpLeosTwampLightEnable OBJECT-TYPE
     SYNTAX             INTEGER {
                            disable(0),
                            enable(1)
                        }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TWAMP Light enable/disable."
     ::= { wwpLeosTwampModule 6 }   

 --
 -- TWAMP Server Test Sessions Status
 --

 wwpLeosTwampServerSessionsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTwampServerSessionEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of Ethernet Ports Traps."
     ::= { wwpLeosTwampModule 7 }
                
 wwpLeosTwampServerSessionEntry OBJECT-TYPE
     SYNTAX       WwpLeosTwampServerSessionEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "TWAMP Server Session characteristics."
     INDEX { wwpLeosTwampServerSessionId }
     ::= { wwpLeosTwampServerSessionsTable 1 } 

 WwpLeosTwampServerSessionEntry ::= SEQUENCE { 
     wwpLeosTwampServerSessionId        INTEGER,
     wwpLeosTwampServerSessionState     INTEGER,     
     wwpLeosTwampServerSessionPort      INTEGER,     
     wwpLeosTwampServerSessionHost      IpAddress,     
     wwpLeosTwampServerSessionNumPkts   Integer32,     
     wwpLeosTwampServerSessionSeqNum    Integer32,
     wwpLeosTwampServerSessionHwAssist  INTEGER     
  } 

 wwpLeosTwampServerSessionId     OBJECT-TYPE
     SYNTAX             INTEGER (1..10)
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Session index for TWAMP Server records."
     ::= { wwpLeosTwampServerSessionEntry 1 }   
     
 wwpLeosTwampServerSessionState   OBJECT-TYPE
     SYNTAX         INTEGER {
                        listen(0),
                        greet(1),
                        start(2),
                        accept(3),
                        test(4),
                        stop(5),
                        error(6)
                    }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "The current state of the Server Session."
     ::= { wwpLeosTwampServerSessionEntry 2 }
     
 wwpLeosTwampServerSessionPort     OBJECT-TYPE
     SYNTAX             INTEGER (0..65535)
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Host source/reply port for TWAMP Server records."
     ::= { wwpLeosTwampServerSessionEntry 3 }   
     
 wwpLeosTwampServerSessionHost     OBJECT-TYPE
     SYNTAX             IpAddress
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Host IP address for TWAMP Server records."
     ::= { wwpLeosTwampServerSessionEntry 4 }   
     
 wwpLeosTwampServerSessionNumPkts     OBJECT-TYPE
     SYNTAX             Integer32 
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Number of packets defined for TWAMP Server records."
     ::= { wwpLeosTwampServerSessionEntry 5 }   
     
 wwpLeosTwampServerSessionSeqNum     OBJECT-TYPE
     SYNTAX             Integer32 
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Current sequence number for TWAMP Server records."
     ::= { wwpLeosTwampServerSessionEntry 6 }   
 
 wwpLeosTwampServerSessionHwAssist   OBJECT-TYPE
     SYNTAX         INTEGER {
                        inactive(0),
                        active(1)
                    }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "The current state of the Server Session FPGA Hardware Assist."
     ::= { wwpLeosTwampServerSessionEntry 7 }
     
 --
 -- TWAMP TCP Session Timeout
 --

  wwpLeosTwampTimeout OBJECT-TYPE
     SYNTAX             INTEGER (1..86400)
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TCP session timeout (max lifetime) for TWAMP messaging."
     ::= { wwpLeosTwampModule 8 }   
     
    
 --
 -- TWAMP Client Test Sessions
 --

 wwpLeosTwampClientSessionsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTwampClientSessionEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of Client Sessions.
             To create an entry set the twampClientSessionStatus to 2 and provide SessionName and 
             set the sessionHost to valid IP Address."
     ::= { wwpLeosTwampModule 9 }
                
 wwpLeosTwampClientSessionEntry OBJECT-TYPE
     SYNTAX       WwpLeosTwampClientSessionEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "TWAMP Client Session characteristics."
     INDEX { wwpLeosTwampClientSessionId }
     ::= { wwpLeosTwampClientSessionsTable 1 } 

 WwpLeosTwampClientSessionEntry ::= SEQUENCE { 
     wwpLeosTwampClientSessionId        INTEGER,
     wwpLeosTwampClientSessionStatus    INTEGER,
     wwpLeosTwampClientSessionName      DisplayString,
     wwpLeosTwampClientSessionHost      IpAddress,     
     wwpLeosTwampClientSessionState     INTEGER,     
     wwpLeosTwampClientSessionCommPort  INTEGER,     
     wwpLeosTwampClientSessionCosPolicy INTEGER,     
     wwpLeosTwampClientSessionDscp      INTEGER,     
     wwpLeosTwampClientSessionIpPrec    INTEGER,     
     wwpLeosTwampClientSessionType      INTEGER,     
     wwpLeosTwampClientSessionPktSize   INTEGER,     
     wwpLeosTwampClientSessionRepeat    INTEGER,     
     wwpLeosTwampClientSessionNumPkts   Integer32,     
     wwpLeosTwampClientSessionSeqNum    Integer32,
     wwpLeosTwampClientSessionRxHw      INTEGER,
     wwpLeosTwampClientSessionTxHw      INTEGER,
     wwpLeosTwampClientSessionDot1dpri  INTEGER     
  } 

 wwpLeosTwampClientSessionId     OBJECT-TYPE
     SYNTAX             INTEGER (1..20)
     MAX-ACCESS         not-accessible
     STATUS             current
     DESCRIPTION
                "Session index for TWAMP Client records."
     ::= { wwpLeosTwampClientSessionEntry 1 }   
     
 wwpLeosTwampClientSessionStatus OBJECT-TYPE
     SYNTAX         INTEGER {
                        active(1),
                        createAndGo(2),
                        clear(3),
                        startTest(4),
                        stopTest(5),
                        clearStats(6)
                    }
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
        "Setting this object to 'createAndGo' will create the entry in the table.       
         Setting this object to 'clear' will clear the entry contents in the table.
         Setting this object to 'startTest' will begin the entry's defined test.
         Setting this object to 'stopTest' will abort the entry's current running test.
         Setting this object to 'clearStats' will clear the statistics for that client session."
     ::= { wwpLeosTwampClientSessionEntry 2 }
 
 wwpLeosTwampClientSessionName OBJECT-TYPE
     SYNTAX      DisplayString (SIZE (0..14))
     MAX-ACCESS  read-write
     STATUS      current
     DESCRIPTION
             "Text string containing the session's unique name."
     ::= { wwpLeosTwampClientSessionEntry 3 }

 wwpLeosTwampClientSessionHost     OBJECT-TYPE
     SYNTAX             IpAddress
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "Host IP address for TWAMP test records."
     ::= { wwpLeosTwampClientSessionEntry 4 }   
     
 wwpLeosTwampClientSessionState   OBJECT-TYPE
     SYNTAX         INTEGER {
                        idle(0),
                        greeting(1),
                        serverStart(2),
                        sessionSetup(3),
                        sessionStart(4),
                        testing(5),
                        stop(6),
                        error(7)
                    }
     MAX-ACCESS     read-write
     STATUS         current
     DESCRIPTION
             "The current state of the Client Session."
     ::= { wwpLeosTwampClientSessionEntry 5 }
     
 wwpLeosTwampClientSessionCommPort     OBJECT-TYPE
     SYNTAX             INTEGER (0..65535)
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "Host source/reply port for TWAMP test records."
     ::= { wwpLeosTwampClientSessionEntry 6 }   
     
 wwpLeosTwampClientSessionCosPolicy     OBJECT-TYPE
     SYNTAX         INTEGER {
                        dscp(1),
                        ipPrec(2)
                    }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "IP class of service to use for test message exchange"
     ::= { wwpLeosTwampClientSessionEntry 7 }   
 
 wwpLeosTwampClientSessionDscp     OBJECT-TYPE
     SYNTAX             INTEGER(0..63) 
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "DSCP value to use for TWAMP test messages."
     ::= { wwpLeosTwampClientSessionEntry 8 }   
 
 wwpLeosTwampClientSessionIpPrec     OBJECT-TYPE
     SYNTAX             INTEGER(0..7) 
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "IP-PREC value to use for TWAMP test messages."
     ::= { wwpLeosTwampClientSessionEntry 9 }   
 
 wwpLeosTwampClientSessionType     OBJECT-TYPE
     SYNTAX         INTEGER {
                        fixed(1),
                        poisson(2)
                    }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TWAMP test session sampling method setting."
     ::= { wwpLeosTwampClientSessionEntry 10 }   
 
 wwpLeosTwampClientSessionPktSize     OBJECT-TYPE
     SYNTAX             INTEGER(64..1500) 
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "IP Packet size to use for TWAMP test messages."
     ::= { wwpLeosTwampClientSessionEntry 11 }   
 
 wwpLeosTwampClientSessionRepeat     OBJECT-TYPE
     SYNTAX         INTEGER {
                        on(1),
                        off(2)
                    }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TWAMP test session continuous mode setting."
     ::= { wwpLeosTwampClientSessionEntry 12 }   
 
 wwpLeosTwampClientSessionSeqNum     OBJECT-TYPE
     SYNTAX             Integer32 
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Current sequence number for TWAMP test messages."
     ::= { wwpLeosTwampClientSessionEntry 13 }   
 
 wwpLeosTwampClientSessionNumPkts     OBJECT-TYPE
     SYNTAX             Integer32 
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Number of packets defined for TWAMP test session."
     ::= { wwpLeosTwampClientSessionEntry 14 } 
     
 wwpLeosTwampClientSessionRxHw   OBJECT-TYPE
     SYNTAX         INTEGER {
                        inactive(0),
                        active(1)
                    }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "The current state of the Client Session FPGA RX Hardware Assist."
     ::= { wwpLeosTwampClientSessionEntry 15 }
     
 wwpLeosTwampClientSessionTxHw   OBJECT-TYPE
     SYNTAX         INTEGER {
                        inactive(0),
                        active(1)
                    }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "The current state of the Client Session FPGA TX Hardware Assist."
     ::= { wwpLeosTwampClientSessionEntry 16 }
     
 wwpLeosTwampClientSessionDot1dpri OBJECT-TYPE
     SYNTAX             INTEGER(0..7) 
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "802.1d priority value to use for TWAMP test messages."
     ::= { wwpLeosTwampClientSessionEntry 17 }   
 
 --
 -- TWAMP Client Test Sessions Statistics Table
 --

 wwpLeosTwampClientSessionsStatisticsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTwampClientSessionStatisticsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of Ethernet Ports Traps."
     ::= { wwpLeosTwampModule 11 }
                
 wwpLeosTwampClientSessionStatisticsEntry OBJECT-TYPE
     SYNTAX       WwpLeosTwampClientSessionStatisticsEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "TWAMP Client Session characteristics."
     INDEX { wwpLeosTwampClientSessionStatsIndex, wwpLeosTwampClientStatsRecordIndex}
     ::= { wwpLeosTwampClientSessionsStatisticsTable 1 } 

 WwpLeosTwampClientSessionStatisticsEntry ::= SEQUENCE { 
     wwpLeosTwampClientSessionStatsIndex        INTEGER,
     wwpLeosTwampClientStatsRecordIndex         INTEGER,
     wwpLeosTwampClientSessionStatsName         DisplayString,
     wwpLeosTwampClientSessionTimestamp         Unsigned32,
     wwpLeosTwampClientSessionStatsPktTx        Unsigned32,
     wwpLeosTwampClientSessionStatsPktRx        Unsigned32,
     wwpLeosTwampClientSessionStatsPktOL        Unsigned32,
     wwpLeosTwampClientSessionStatsPktRL        Unsigned32,
     wwpLeosTwampClientSessionStatsRTMin        Unsigned32,
     wwpLeosTwampClientSessionStatsRTMax        Unsigned32,
     wwpLeosTwampClientSessionStatsRTMean       Unsigned32,
     wwpLeosTwampClientSessionStatsRTStdDev     Unsigned32,
     wwpLeosTwampClientSessionStatsRT95th       Unsigned32,
     wwpLeosTwampClientSessionStatsRT99pt9th    Unsigned32,
     wwpLeosTwampClientSessionStatsOWOMin       Unsigned32,
     wwpLeosTwampClientSessionStatsOWOMax       Unsigned32,
     wwpLeosTwampClientSessionStatsOWOMean      Unsigned32,
     wwpLeosTwampClientSessionStatsOWOStdDev    Unsigned32,
     wwpLeosTwampClientSessionStatsOWO95th      Unsigned32,
     wwpLeosTwampClientSessionStatsOWO99pt9th   Unsigned32,
     wwpLeosTwampClientSessionStatsOWBMin       Unsigned32,
     wwpLeosTwampClientSessionStatsOWBMax       Unsigned32,
     wwpLeosTwampClientSessionStatsOWBMean      Unsigned32,
     wwpLeosTwampClientSessionStatsOWBStdDev    Unsigned32,
     wwpLeosTwampClientSessionStatsOWB95th      Unsigned32,
     wwpLeosTwampClientSessionStatsOWB99pt9th   Unsigned32,
     wwpLeosTwampClientSessionStatsTPMin        Unsigned32,
     wwpLeosTwampClientSessionStatsTPMax        Unsigned32,
     wwpLeosTwampClientSessionStatsTPMean       Unsigned32,
     wwpLeosTwampClientSessionStatsTPStdDev     Unsigned32,
     wwpLeosTwampClientSessionStatsTP95th       Unsigned32,
     wwpLeosTwampClientSessionStatsTP99pt9th    Unsigned32
  } 

 wwpLeosTwampClientSessionStatsIndex     OBJECT-TYPE
     SYNTAX             INTEGER (1..20)
     MAX-ACCESS         not-accessible
     STATUS             current
     DESCRIPTION
                "Session index for TWAMP Server records."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 1 }   
     
 wwpLeosTwampClientStatsRecordIndex     OBJECT-TYPE
     SYNTAX             INTEGER (1..96)
     MAX-ACCESS         not-accessible
     STATUS             current
     DESCRIPTION
                "Session index for TWAMP Client Statistics records."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 2 }   
     
 wwpLeosTwampClientSessionStatsName OBJECT-TYPE
     SYNTAX             DisplayString (SIZE (0..14))
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
             "Text string containing the session's unique name."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 3 }

 wwpLeosTwampClientSessionTimestamp     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "The time at which this statistics record was generated - Unix epoch seconds."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 4 }   

 wwpLeosTwampClientSessionStatsPktTx     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "The number of test packets emitted."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 5 }   

 wwpLeosTwampClientSessionStatsPktRx     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "The number of test packets received."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 6 }   

 wwpLeosTwampClientSessionStatsPktOL     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "The number of test packets lost one-way."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 7 }   

 wwpLeosTwampClientSessionStatsPktRL     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "The number of test packets lost round-trip."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 8 }   

 wwpLeosTwampClientSessionStatsRTMin     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Round trip minimum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 9 }   

 wwpLeosTwampClientSessionStatsRTMax     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Round trip maximum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 10 }   

 wwpLeosTwampClientSessionStatsRTMean     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Round trip average interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 11 }   

 wwpLeosTwampClientSessionStatsRTStdDev     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Round trip standard deviation (jitter)."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 12 }   

 wwpLeosTwampClientSessionStatsRT95th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Round trip 95th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 13 }   

 wwpLeosTwampClientSessionStatsRT99pt9th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Round trip 99.9th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 14 }   

 wwpLeosTwampClientSessionStatsOWOMin     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way out minimum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 15 }   

 wwpLeosTwampClientSessionStatsOWOMax     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way out maximum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 16 }   

 wwpLeosTwampClientSessionStatsOWOMean     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way out average interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 17 }   

 wwpLeosTwampClientSessionStatsOWOStdDev     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way out standard deviation (jitter)."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 18 }   

 wwpLeosTwampClientSessionStatsOWO95th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way out 95th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 19 }   

 wwpLeosTwampClientSessionStatsOWO99pt9th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way out 99.9th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 20 }   

 wwpLeosTwampClientSessionStatsOWBMin     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way back minimum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 21 }   

 wwpLeosTwampClientSessionStatsOWBMax     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way back maximum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 22 }   

 wwpLeosTwampClientSessionStatsOWBMean     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way back average interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 23 }   

 wwpLeosTwampClientSessionStatsOWBStdDev     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way back standard deviation (jitter)."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 24 }   

 wwpLeosTwampClientSessionStatsOWB95th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way back 95th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 25 }   

 wwpLeosTwampClientSessionStatsOWB99pt9th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "One way back 99.9th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 26 }   

 wwpLeosTwampClientSessionStatsTPMin     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Target processing minimum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 27 }   

 wwpLeosTwampClientSessionStatsTPMax     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Target processing maximum interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 28 }   

 wwpLeosTwampClientSessionStatsTPMean     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Target processing average interval."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 29 }   
 
 wwpLeosTwampClientSessionStatsTPStdDev     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Target processing standard deviation (jitter)."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 30 }   

 wwpLeosTwampClientSessionStatsTP95th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Target processing 95th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 31 }   

 wwpLeosTwampClientSessionStatsTP99pt9th     OBJECT-TYPE
     SYNTAX             Unsigned32
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Target processing 99.9th percentile."
     ::= { wwpLeosTwampClientSessionStatisticsEntry 32 }   

 --
  --  Added TWAMP Fields
 --

 wwpLeosTwampClientDscp     OBJECT-TYPE
     SYNTAX             INTEGER(0..63) 
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "DSCP value to use for TWAMP Client TCP test messages."
     ::= { wwpLeosTwampModule 12 }   
 
 wwpLeosTwampServerDscp     OBJECT-TYPE
     SYNTAX             INTEGER(0..63) 
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "DSCP value to use for TWAMP Server TCP test messages."
     ::= { wwpLeosTwampModule 13 }   
 
 wwpLeosTwampClientHwAssist     OBJECT-TYPE
     SYNTAX         INTEGER {
                        on(1),
                        off(2)
                    }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TWAMP Client hardware assist setting."
     ::= { wwpLeosTwampModule 14 }   
 
 wwpLeosTwampServerHwAssist     OBJECT-TYPE
     SYNTAX         INTEGER {
                        on(1),
                        off(2)
                    }
     MAX-ACCESS         read-write
     STATUS             current
     DESCRIPTION
                "TWAMP Server hardware assist setting."
     ::= { wwpLeosTwampModule 15 }   
 

 --
 -- TWAMP Server Control Sessions Status
 --

 wwpLeosTwampServerCtrlSessionsTable OBJECT-TYPE
     SYNTAX       SEQUENCE OF WwpLeosTwampServerCtrlSessionEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "Table of TWAMP Control Session Records."
     ::= { wwpLeosTwampModule 16 }
                
 wwpLeosTwampServerCtrlSessionEntry OBJECT-TYPE
     SYNTAX       WwpLeosTwampServerCtrlSessionEntry
     MAX-ACCESS   not-accessible
     STATUS       current
     DESCRIPTION
             "TWAMP Server Control Session characteristics."
     INDEX { wwpLeosTwampServerCtrlSessionId }
     ::= { wwpLeosTwampServerCtrlSessionsTable 1 } 

 WwpLeosTwampServerCtrlSessionEntry ::= SEQUENCE { 
     wwpLeosTwampServerCtrlSessionId        INTEGER,
     wwpLeosTwampServerCtrlSessionState     INTEGER,     
     wwpLeosTwampServerCtrlSessionPort      INTEGER,     
     wwpLeosTwampServerCtrlSessionHost      IpAddress,
     wwpLeosTwampServerCtrlSessionTestMap   INTEGER     
  } 

 wwpLeosTwampServerCtrlSessionId     OBJECT-TYPE
     SYNTAX             INTEGER (1..10)
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Session index for TWAMP Server Control Session records."
     ::= { wwpLeosTwampServerCtrlSessionEntry 1 }   
     
 wwpLeosTwampServerCtrlSessionState   OBJECT-TYPE
     SYNTAX         INTEGER {
                        listen(0),
                        greet(1),
                        start(2),
                        accept(3),
                        test(4),
                        stop(5),
                        error(6)
                    }
     MAX-ACCESS     read-only
     STATUS         current
     DESCRIPTION
             "The current state of the Server Control Session."
     ::= { wwpLeosTwampServerCtrlSessionEntry 2 }
     
 wwpLeosTwampServerCtrlSessionPort     OBJECT-TYPE
     SYNTAX             INTEGER (0..65535)
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Host port for TWAMP Server Control session records."
     ::= { wwpLeosTwampServerCtrlSessionEntry 3 }   
     
 wwpLeosTwampServerCtrlSessionHost     OBJECT-TYPE
     SYNTAX             IpAddress
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Host IP address for TWAMP Server Control session records."
     ::= { wwpLeosTwampServerCtrlSessionEntry 4 }   
     
 wwpLeosTwampServerCtrlSessionTestMap     OBJECT-TYPE
     SYNTAX             INTEGER (0..65535) 
     MAX-ACCESS         read-only
     STATUS             current
     DESCRIPTION
                "Bitmap of TWAMP Test sessions associated with Control session."
     ::= { wwpLeosTwampServerCtrlSessionEntry 5 }   
     
 --

 END

 
