Configuring TFTP

You can configure the TFTP credentials for the switch.

1. From the menu bar, choose Admin > General > SFTP/TFTP Credentials.
You see the SFTP/TFTP credentials page.

2. In the Server Type field, use the radio button to select TFTP.

3. From the Verification Switch drop-down, select the switch.

4. Click Apply to apply the configuration.

5. Click Apply and Verify to apply and verify the configuration.

Note Ensure that no TFTP server is running on the server machine. FMS internal TFTP server will be used for all backup operations.