> # Configuring Fabric Names

> ## Detailed Steps

> To set the fabric name value for a disabled fcdomain, follow these steps:

> 1. Expand Fabric > All VSANs and then select Domain Manager in the Logical Domains pane for the fabric and VSAN that you want to set the fabric name for.

> You see the running configuration of the domain in the Information pane.

> 2. Click the Configuration tab and set the fabric name for each switch in the fabric.
> 3. Click the Apply Changes icon to save these changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.