> # Fabric Binding Statistics

> Field | Description
> --- | ---
> AllowedReqs | The number of requests from switches to become part of the fabric that have been allowed on this VSAN/VLAN.
> DeniedReqs | The number of requests from switches to become part of the fabric that have been denied on this VSAN/VLAN.
> Clear | When set to clear, it results in fabric bind statistic counters being cleared on this VSAN/VLAN.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.