> # IPSEC Tunnels

> Field | Description
> --- | ---
> Local Address | The IP address of the local endpoint for the IPsec Phase-2 tunnel.
> RemoteAdddress | The type of the IP address of the remote endpoint for the IPsec Phase-2 tunnel.
> ESP Encryption | The encryption algorithm used by the outbound security association of the IPsec Phase-2 tunnel.
> ESP Encryption KeySize | The key size in bits of the negotiated key to be used with the algorithm denoted by ceipSecTunOutSaEncryptAlgo. For DES and 3DES the key size is respectively 56 and 168. For AES, this will denote the negotiated key size.
> ESP Authentication | The authentication algorithm used by the inbound encapsulation security protocol (ESP) security association of the IPsec Phase-2 tunnel.
> LifeSize (KB) | The negotiated life size of the IPSEC Phase-2 tunnel in kilobytes.
> LifeTime (sec) | The negotiated lifetime of the IPSEC Phase-2 tunnel in seconds. If the tunnel was setup manually, the value of this MIB element should be 0.
> Action | The status of the MIB table row.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.