> # Monitor SVC Session FCP

> The Monitor dialog boxes have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> Cmds | Number of incoming FCP Command frames in this session.
> XferRdys | Number of incoming FCP Transfer Ready frames in this session.
> DataFrames | Number of incoming FCP Data frames.
> Status | Number of incoming FCP status frames.
> DataBytes | Number of incoming FCP Data bytes.
> OverRuns | Number of incoming FCP Overrun frames in this session.
> UnderRuns | Number of incoming FCP Underrun frames in this session.
> Cmds | Number of outgoing FCP Command frames in this session.
> XferRdys | Number of outgoing FCP Transfer Ready frames in this session.
> DataFrames | Number of outgoing FCP Data frames.
> Status | Number of outgoing FCP status frames.
> DataBytes | Number of outgoing FCP Data bytes.
> OverRuns | Number of outgoing FCP OverRun frames in this session.
> UnderRuns | Number of outgoing FCP UnderRun frames in this session.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.