> # Restarting a Domain

> ## Detailed Steps

> To restart the fabric disruptively or nondisruptively, follow these steps:

> 1. Expand Fabric > All VSANs and then select Domain Manager in the Logical Domains pane for the fabric and VSAN that you want to restart.
> 2. Click the Configuration tab.
> 3. Set the Restart drop-down menu to disruptive or nonDisruptive for any switch in the fabric that you want to restart the fcdomain.
> 4. Click the Apply Changes icon to initiate this fcdomain restart.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.