> # Configuring the Default State for Port Prohibiting

> By default, port prohibiting is disabled on the implemented interfaces on the switch. As of Cisco MDS SAN-OS Release 3.0(2), you can change the default port prohibiting state to enabled in VSANs that you create and then selectively disable port prohibiting on implemented ports, if desired. Also, only the FICON configuration files created after you change the default have the new default setting (see the "FICON Configuration Files" topic).

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.