## Configuring Cisco DCNM-SAN Server Properties

To configure Cisco DCNM-SAN Server properties

1. From the menu bar, choose Admin > General > Server Properties.

2. Follow the on-screen instructions and click Apply to confirm the changes.

While connecting to some switches if the connection is getting timed out, in the #CLI session channel type, change default the cli.channel.type value from exec to shell.

Note After configuring the server properties, you need to restart the DCNM server only if you receive a notification stating that the server must be restarted.