> # Fabric Binding Actions

> Field | Description
> --- | ---
> Action | activate - results in the valid fabric bindings on this VSAN/VLAN being activated. activate (Turn Learning Off) - results in the valid fabric bindings on this VSAN/VLAN being activated and copied to the active database and will also result in auto learn being turned off on this VSAN/VLAN, once the activation is complete. force activate - results in forced activation, even if there are errors during activation and the activated fabric bindings will be copied to the active database. force activate (Turn Learning Off) - results in forced activation along with turning auto learn off after activation and the activated fabric bindings will be copied to the active database. deactivate - results in deactivation of currently activated valid fabric bindings (if any), on this VSAN/VLAN. Currently active entries (if any), which would have been present in the active database, will be removed. activation will not be allowed on a VSAN if auto-learn is enabled on that VSAN.
> Enabled | The state of activation on this VSAN/VLAN. If true, then an activation has been attempted as the most recent operation on this VSAN/VLAN. If false, then an activation has not been attempted as the most recent operation on this VSAN/VLAN.
> Result | Indicates the outcome of the most recent activation/deactivation.
> LastChange | When the valid fabric bindings on this VSAN/VLAN were last activated. If the last activation took place prior to the last re-initialization of the agent, then this value will be N/A.
> CopyActive ToConfig | If enabled, results in the active fabric binding database to be copied on to the configuration database on this VSAN/VLAN. Note that the learned entries are also copied.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.