> # Configuring VSAN Membership for iSCSI Hosts

> Individual iSCSI hosts can be configured to be in a specific VSAN. The specified VSAN overrides the iSCSI interface VSAN membership.

> ## Detailed Steps

> To assign VSAN membership for iSCSI hosts, follow these steps:

> 1. Choose End Devices > iSCSI in the Physical Attributes pane.

> You see the iSCSI tables in the Information pane.

> 2. Click the Initiators tab.

> You see the iSCSI initiators configured.

> 3. Fill in the VSAN Membership field to assign a VSAN to the iSCSI hosts.
> 4. Click the Apply Changes icon to save these changes.

> Note When an initiator is configured in any other VSAN (other than VSAN 1), for example VSAN 2, the initiator is automatically removed from VSAN 1. If you also want it to be present in VSAN 1, you must explicitly configure the initiator in VSAN 1.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.