> # Port Security Active Database

> Field | Description
> --- | ---
> Interface or fWWN | The address of a port on the local device.
> Type | The mechanism to identify a switch port.== fwwn - the local switch port is identified by Fabric WWN(fWWN). == intfIndex - the local switch port is identified by ifIndex. == wildCard - wild card (any switch port on local device).
> WWN | Represents the logging in device address.
> IsLearnt | Indicates if this entry is a learnt entry or not.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.