## Deleting Switches From a SME Cluster

Prerequisites

• If the cluster includes more than one switch, you must delete all non-master switches first. It is not possible to delete the master switch from a cluster without first deleting all non-master switches.

Detailed Steps

To delete a switch from a cluster, follow these steps:

1. Click Members to display the switches that are part of the cluster.

2. Select the switch and click Remove.

3. Click OK to delete the switch.

4. View the notification that the switch was deleted.

Note The interface and the node are both removed.