> # Disabling FSPF for Specific Interfaces

> You can disable the FSPF protocol for selected interfaces. By default, FSPF is enabled on all E ports and TE ports. This default can be disabled by setting the interface as passive.

> You can disable the FSPF protocol for selected interfaces. By default, FSPF is enabled on all E ports and TE ports. This default can be disabled by setting the interface as passive.

> ## Detailed Steps

> To disable FSPF for a specific interface, follow these steps:

> 1. Expand Switches, expand FC Interfaces, and then select Physical.

> You see the interface configuration in the Information pane.

> 2. Click the FSPF tab.

> You see the FSPF interface configuration in the Information pane.

> 3. Set a switch Admin Status drop-down menu to down.
> 4. Click Apply Changes to save these changes, or click Undo Changes to discard any unsaved changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.