> # FICON Port Configuration

> Field | Description
> --- | ---
> Show Installed Ports Only | If true, only physically available ports will be listed in the table.
> ESCON Style | ESCON Style Port Configuration display is the Port Configuration table in DM displaying the ESCON Style Ports. In the table, A represents the available ports and P represents the prohibited ports.
> Port/ Prohibit | Enter the FICON address of the port and the prohibited list. (This is an alternative to the table grid.)
> Name | The port name of this port.
> Block | If true, this port will be isolated.
> Prohibit Grid | Click on the grid to add or remove the ability of ports to communicate with each other.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.