> # Enabling CFS for an Application

> All CFS-based applications provide an option to enable or disable the distribution capabilities. Features that existed prior to Cisco SAN-OS Release 2.0(1b) have the distribution capability disabled by default and must have distribution capabilities enabled explicitly.

> Applications introduced in Cisco SAN-OS Release 2.0(1b) or later, or MDS NX-OS Release 4.1(1) or later have the distribution enabled by default.

> The application configuration is not distributed by CFS unless distribution is explicitly enabled for that application.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.