> # Modifying the Device Grouping

> Because not all devices are capable of responding to FC-GS-3 requests, different ports of a single server or storage subsystem may be displayed as individual end devices on the Cisco DCNM-SAN map.

> ## DETAILED STEPS

> 1. Expand End Devices and then choose Storage or Hosts in the Physical Attributes pane.

> You see the end devices displayed in the Information pane.

> 2. Click one of the devices in the Fabric pane, or click the Enclosures tab of the Information pane, and then click the device name (in the Name field) that you want to include in the enclosure.
> 3. Enter a name to identify the new enclosure in the Fabric pane map.
> 4. Click once on the device name in the Name field. To select more than one name, press the Shift key and click each of the other names.
> 5. Press Ctrl-C to copy the selected name(s).
> 6. Press Ctrl-V to paste the device name into the Name field.

> Note To remove devices from an enclosure, triple click the device name and press Delete. To remove an enclosure, repeat this step for each device in the enclosure.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.