> # Port Security Database Differences

> Field | Description
> --- | ---
> CompareWith | Specifies the database for the comparison. configDb - compares the configuration database with respect to active database on this VSAN/VLAN. So, the active database will be the reference database and the results of the difference operation will be with respect to the active database. activeDb - compares the active database with respect to configuration database on this VSAN/VLAN. So, the configuration database will be the reference database and the results of the difference operation will be with respect to the configuration database.
> VSANId | The ID of the VSAN to compare against.
> Interface/fWWN | The address of a port on the local device.
> Type | The mechanism to identify a switch port. fwwn - the local switch port is identified by Fabric WWN(fWWN). intfIndex - the local switch port is identified by ifIndex. wildCard - wild card (any switch port on local device).
> WWN | Represents the logging in device address.
> Reason | Indicates the reason for the difference between the databases being compared, for this entry.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.