Selecting Transport Settings

To enable transport settings in the Transport Settings screen, click On. If Transport Settings is enabled, specify the Trust Point from the drop-down menu.

For more information about trust points, see the IP Services Configuration Guide, Cisco DCNM for SAN and the Cisco MDS 9000 Family NX-OS IP Services Configuration Guide.

If On is selected in the Transport Settings list, SSL is enabled on KMC with the following results:

• New clusters are created. If Off is selected, cluster creation fails.

• Previously created clusters are updated by enabling SSL with trustpoint on the switches. KMC server connection state remains as none until the cluster is updated.

To disable transport settings, click Off.