> # Adding Members to Aliases

> ## Detailed Steps

> To add a member to an alias, follow these steps:

> 1. Choose Zone > Edit Local Full Zone Database.

> You see the Select VSAN dialog box.

> 2. Select a VSAN and click OK.

> You see the Edit Local Full Zone Database dialog box for the selected VSAN.

> 3. Select the member(s) you want to add from the Fabric pane and click Add to Alias or click the alias where you want to add members and click the Insert icon.

> You see the Add Member to Alias dialog box.

> Note The Device Alias radio button is visible only if device alias is in enhanced mode. For more information, see "Creating Device Aliases" topic.

> 4. Click the browse button and select a port name or check the LUN check box and click the browse button to configure LUNs.
> 5. Click Add to add the member to the alias.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.