> # PKI Trust Point Actions

> Field | Description
> --- | ---
> Name | The name or label of the trust point action.
> Command | The PKI support action to be triggered for this trust point entry.
> Url | Indicates the file name containing the input or output certificate data needed for the PKI support action being triggered on this entry. The file name should be specified as bootflash:<filename> and it should be available on bootflash or get created on bootflash depending upon the action being triggered.
> Password | Indicates the password required to perform the PKI support action being triggered. This password is required to be specified only for certreq, importpkcs12 and exportpkcs12 actions. For security reasons, the value, whenever it is retrieved by the management protocol, is always the zero length string.
> Last Command | The PKI support action attempted last. The value attempted to be set for cpkiAction object last. If no action has been triggered for the trust point after its creation, then retrieving the value of this object will return none.
> Result | The result of the execution of the last PKI support action.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.