> # Domain Manager Allowed DomainIds

> Field | Description
> --- | ---
> List | Provides the lists of domains that are allowed. A domain is allowed in this VSAN if the corresponding bit has a value of 1. If it has a value which is less than 32 bytes long, then the domains which are not represented are not considered to be in the list. If this object is a zero-length string, then no domains are allowed in this VSAN.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.