> # About iSCSI Configuration Limits

> iSCSI configuration has the following limits:

> - The maximum number of iSCSI and iSLB initiators supported in a fabric is 2000.
> - The maximum number of iSCSI and iSLB initiators supported is 200 per port.
> - The maximum number of iSCSI and iSLB sessions supported by an IPS port in either transparent or proxy initiator mode is 500.
> - The maximum number of iSCSI and iSLB session support by switch is 5000.
> - The maximum number of iSCSI and iSLB targets supported in a fabric is 6000.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.