## Converting Disks to Signature Mode

To convert a cluster to signature mode, follow these steps:

1. In DCNM-SAN Web Client, click the SME tab.

2. Select Clusters in the navigation pane. Click and expand on the desired destination clusters.

The Cluster Details screen is displayed.

3. Click Convert Disks to Signature Mode.

The Signature Mode Conversion screen is displayed.

4. Click Next.

The Convert Cluster screen is displayed.