> # Statistics SCSI Sense Errors

> Field | Description
> --- | ---
> NotRdyErrs | The number of NOT READY SCSI SENSE key errors received on this LUN on this flow. This indicates that the logical unit being addressed cannot be accessed.
> MedErrs | The number of MEDIUM ERROR SCSI SENSE key errors received on this LUN on this flow. This indicates that the command terminated with a non-recovered error condition possibly caused by a flaw in the medium.
> HwErrs | The number of HARDWARE ERROR SCSI SENSE key errors received on this LUN on this flow. This indicates that the target detected a non-recoverable hardware failure.
> IllReqErrs | The number of ILLEGAL REQUEST SCSI SENSE key errors received on this LUN on this flow.
> UnitAttErrs | The number of UNIT ATTENTION SCSI SENSE key errors received on this LUN on this flow.
> DatProtErrs | The number of DATA PROTECT SCSI SENSE key errors received on this LUN on this flow.
> BlankErrs | The number of BLANK CHECK SCSI SENSE key errors received on this LUN on this flow.
> CpAbrtErrs | The number of COPY ABORTED SCSI SENSE key errors received on this LUN on this flow.
> AbrtCmdErrs | The number of ABORTED COMMAND SCSI SENSE key errors received on this LUN on this flow.
> VolFlowErrs | The number of VOLUME OVERFLOW SCSI SENSE key errors received on this LUN on this flow.
> MiscmpErrs | The number of VOLUME OVERFLOW SCSI SENSE key errors received on this LUN on this flow.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.