> # WWN Manager

> Field | Description
> --- | ---
> SwitchWWN | The World-Wide Name of this fabric element. It's a 64-bit identifier and is unique worldwide.
> Type 1 WWNs
> Max | Maximum number of NAA Type 1 WWNs that are available for assignment to internal entities.
> Available | Number of NAA Type 1 WWNs that are currently available for assignment to internal entities.
> Reserved | Number of NAA Type 1 WWNs that are reserved for internal purposes.
> Type 2 & 5 WWNs
> Max | Maximum number of total WWNs of types NAA Type 2 and Type 5 WWNs available for assignment to internal entities.
> Available | Sum of number of NAA Type 2 and Type 5 WWNs currently available for assignment to the internal entities.
> Reserved | Number of total WWNs of types NAA Type 2 and Type 5 WWNs reserved for internal purposes.
> Enable Secondary when more WWWNs needed
> BaseMacAddress | The first MAC address used for generating World Wide Names (WWNs) when the default range of WWNs generated from supervisor MAC address are exhausted.
> MacAddressRange | The number of secondary MAC Addresses starting from and including the wwnmSecondayBaseMacAddress.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.