> # IP Statistics SNMP

> Field | Description
> --- | ---
> BadVersions | The total number of SNMP messages which were delivered to the SNMP entity and were for an unsupported SNMP version.
> BadCommunityNames | The total number of SNMP messages delivered to the SNMP entity which used a SNMP community name not known to said entity.
> BadCommunityUses | The total number of SNMP messages delivered to the SNMP entity which represented an SNMP operation which was not allowed by the SNMP community named in the message.
> ASNParseErrs | The total number of ASN.1 or BER errors encountered by the SNMP entity when decoding received SNMP messages.
> TooBigs | The total number of SNMP PDUs which were delivered to the SNMP protocol entity and for which the value of the error-status field is tooBig.
> SilentDrops | The total number of GetRequest-PDUs, GetNextRequest-PDUs, GetBulkRequest-PDUs, SetRequest-PDUs, and InformRequest-PDUs delivered to the SNMP entity which were silently dropped because the size of a reply containing an alternate Response-PDU with an empty variable-bindings field was greater than either a local constraint or the maximum message size associated with the originator of the request.
> ProxyDrops | The total number of GetRequest-PDUs, GetNextRequest-PDUs, GetBulkRequest-PDUs, SetRequest-PDUs, and InformRequest-PDUs delivered to the SNMP entity which were silently dropped because the transmission of the (possibly translated) message to a proxy target failed in a manner (other than a time-out) such that no Response-PDU could be returned.
> NoSuchNames | The total number of SNMP PDUs which were delivered to the SNMP protocol entity and for which the value of the error-status field is noSuchName.
> BadValues | The total number of SNMP PDUs which were delivered to the SNMP protocol entity and for which the value of the error-status field is badValue.
> ReadOnlys | The total number valid SNMP PDUs which were delivered to the SNMP protocol entity and for which the value of the error-status field is readOnly. It should be noted that it is a protocol error to generate an SNMP PDU which contains the value readOnly in the error-status field, as such this is provided as a means of detecting incorrect implementations of the SNMP.
> GenErrs | The total number of SNMP PDUs which were delivered to the SNMP protocol entity and for which the value of the error-status field is genErr.
> Pkts | The total number of messages delivered to the SNMP entity from the transport service.
> GetRequests | The total number of SNMP Get-Request PDUs which have been accepted and processed by the SNMP protocol entity.
> GetNexts | The total number of SNMP Get-Next PDUs which have been accepted and processed by the SNMP protocol entity.
> SetRequests | The total number of SNMP Set-Request PDUs which have been accepted and processed by the SNMP protocol entity.
> OutTraps | The total number of SNMP Trap PDUs which have been generated by the SNMP protocol entity.
> OutGetResponses | The total number of SNMP Get-Response PDUs which have been generated by the SNMP protocol entity.
> OutPkts | The total number of SNMP Messages which were passed from the SNMP protocol entity to the transport service.
> TotalReqVars | The total number of MIB objects which have been retrieved successfully by the SNMP protocol entity as the result of receiving valid SNMP Get-Request and Get-Next PDUs.
> TotalSetVars | The total number of MIB objects which have been altered successfully by the SNMP protocol entity as the result of receiving valid SNMP Set-Request PDUs.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.