Exporting Volume Groups Using Standard Mode

Detailed Steps

To export a volume group from a deactivated cluster (Standard security mode), follow these steps:

1. Select Volume Groups (in a deactivated cluster) to display the volume groups in the cluster. Select a volume group and click Export.

2. Insert one of the five smart cards into the smart card reader. Click Next.

3. Enter the smart card Label and PIN. Click Next.

4. Enter the password to encrypt the volume group file. Confirm the password and click Next.

5. Click Download to begin downloading the file.

6. You will be asked if you want to open or save the file. To save the file, click Save.