Replacing Smart Cards Using Standard Mode

In Standard security mode, the master key can be downloaded to a replacement smart card from the DCNM-SAN Web Client.

Detailed Steps

To replace a smart card (Standard security mode), follow these steps:

1. Select Smartcards to display the smart card information for the cluster.

2. Click Replace to launch the smart card replacement wizard. Click Next.

3. Insert the smart card and enter the Password, PIN, and Label for the smart card. Click Next.

4. Click Finish to close the wizard.