> # IPSEC CryptoMap Set Entry

> Field | Description
> --- | ---
> IpFilter | Specifies an IP protocol filter to be secured using this cryptomap entry. When it has a value of zero-length string, it is not valid/applicable.
> TransformSetIdList | The list of cipsXformSetId that are members of this CipsStaticCryptomapEntry. The value of this object is a concatenation of zero ormore 4-octet strings, where each 4-octet string contains a 32-bit cipsXformSetId value in network byte order. A zero length string value means this list has no members.
> AutoPeer | If true the destination address is taken as the peer address, while creating the tunnel.
> Peer Address | The IP address of the peer to which this cryptomap entry is currently connected.
> PFS | Identifies whether the tunnels instantiated due to this policy item should use Perfect Forward Secrecy (PFS) and if so, what group of Oakley they should use.
> LifeTime | Specifies the lifetime of the IPsec Security Associations (SA) created using this IPsec policy entry.
> Lifesize Value | Identifies the life size (maximum traffic in bytes that may be carried) of the IPSec SAs created using this IPSec policy entry. When a Security Association (SA) is created using this IPsec policy entry, its life size takes the value of this object.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.