## Configuring CFS Regions For FC-Redirect

To configure the CFS regions for FC-Redirect, do the following tasks:

1. Configure a switch in the CFS region as shown in the following example:

switch# config t

switch# cfs region 2

switch# fc-redirect

switch# end

Repeat this step for all the switches that are included in the specified region.

2. Confirm all the required switches are available in the CFS region by entering the show fc-redirect peer-switches command.

3. To migrate existing SME installations to CFS regions for FC-Redirect, delete all the existing FC-Redirect configurations created by the switches in other regions from each switch. To remove the configurations, perform the following steps:

a. Obtain a list of all FC-Redirect configurations by entering the show fc-redirect configs.

b. Remove all configurations created by the switches in other regions by using the clear fc-redirect configs command. The configurations are removed from the switches but the switches remain active in the region in which they are created.