> # Deleting IP-ACLs

> ## Prerequisites

> You must delete the association between the IP-ACL and interfaces before deleting the IP-ACL.

> ## Detailed Steps

> To delete an IP-ACL, follow these steps:

> 1. Expand Switches > Security, and then select IP ACL from the Physical Attributes pane.

> You see the IP-ACL configuration in the Information pane.

> 2. Click the Profiles tab.

> You see a list of switches, ACLs, and profile names.

> 3. Select the row you want to delete. To delete multiple rows, hold down the Shift key while selecting rows.
> 4. Click Delete Row. The IP-ACLs are deleted.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.