> # Configuring Transform Sets

> ## Detailed Steps

> To configure transform sets, follow these steps:

> 1. Expand Switches > Security, and then select IPSec in the Physical Attributes pane.
> 2. Click the Transform Set tab in the Information pane.
> 3. Click Create Row.

> You see the Create IPSEC dialog box.

> 4. Select the switches that you want to create a transform set for in the Create Transform Set dialog box.
> 5. Assign a name and protocol for the transform set.
> 6. Select the encryption and authentication algorithm. See Table 36-2 to verify the allowed transform combinations.
> 7. Click Create to create the transform set or you click Close.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.