> # Configuring Event Security

> SNMP events can be secured against interception or eavesdropping in the same way that SNMP messages are secured. DCNM-SAN or Device Manager allow you to configure the message processing model, the security model, and the security level for the SNMP events that the switch generates.

> ## Restrictions

> - This is an advanced function that should only be used by administrators having experience with SNMPv3.

> ## Detailed Steps

> To configure SNMP event security, follow these steps:

> 1. Expand Events and then select SNMP Traps.
> 2. Click the Security tab in the Information pane.

> You see the security information for SNMP notifications.

> 3. Set the message protocol model (MPModel), security model, security name, and security level.
> 4. Click the Apply Changes icon to save and apply your changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.