> # FC Interface Monitor FICON

> The Monitor dialog boxes have special Monitor Dialog Controls.

> Field | Description
> --- | ---
> FramePacingTime | Number of 2.5 microsecond units that frame transmission is blocked due to zero credit.
> DispErrorsInFrame | Number of frames with disparity errors.
> EOFErrs | Number of frames with EOF errors.
> DispErrsOutOfFrame | Number of frames with OOF errors.
> InvalidOrderSets | Number of invalid or unrecognizable Order Sets outside of frames.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.