> # Discarding the Distribution Session

> Discarding the distribution of a session in progress causes the configuration in the temporary buffer to be dropped. The distribution is not applied.

> ## Detailed Steps

> To discard RADIUS or TACACS+ distribution, follow these steps:

> 1. Expand Switches > Security > AAA, and then select either RADIUS or TACACS+. You see either the RADIUS or TACACS+ configuration in the Information pane.
> 2. Click the CFS tab. You see either the RADIUS or TACACS+ CFS configuration.
> 3. Choose abort from the Config Action drop-down list for each switch that should discard the pending RADIUS or TACACS+ distribution.
> 4. Click Apply Changes.
> .

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.