> # Converting Zone Members to pWWN-based Members

> You can convert zone and alias members from switch port or FC ID- based membership to pWWN-based membership. You can use this feature to convert to pWWN so that your zone configuration does not change if a card or switch is changed in your fabric.

> ## Detailed Steps

> To convert switch port and FC ID members to pWWN members, follow these steps:

> 1. Choose Zone > Edit Local Full Zone Database.

> You see the Select VSAN dialog box.

> 2. Select a VSAN and click OK.

> You see the Edit Local Full Zone Database dialog box for the selected VSAN.

> 3. Click the zone you want to convert.
> 4. Choose Tools > Convert Switch Port/FCID members to By pWWN.

> You see the conversion dialog box, which lists all members that will be converted.

> 5. Verify the changes and click Continue Conversion.
> 6. Click Yes in the confirmation dialog box to convert that member to pWWN-based membership.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.